# Clifton Cameras Product Specification

## Sony FE 100mm f2.8 STF GM OSS Lens Full Spec

Mount: Sony E-mount  
Format: 35mm full frame  
Focal Length (mm): 100  
35mm Equivalent Focal Length (APS-C): 150  
Lens Groups / Elements: 10-13 \*excluding APD element  
Angle of View (35mm): 24°  
Angle of View (APS-C): 16°1  
Maximum Aperture (F): F2.8 (T5.6)  
Minimum Aperture (F): F20 (T22)  
Aperture Blades: 11  
Circular Aperture: Yes  
Minimum Focus Distance: 0.85m / 2.79 ft. (at "0.85m-∞" position); 0.57m / 1.87 ft. (at "0.57m-1.0m" position)  
Maximum Magnification Ratio (X): 0.14 (at "0.85m-∞" position); 0.25 (at "0.57m-1.0m" position)  
Filter Diameter (mm): 72  
Image Stabilization (SteadyShot): Optical SteadyShot  
Teleconverter Compatibility (X1.4): -  
Teleconverter Compatibility (X2.0): -  
Hood Type: Round shape, bayonet type

Size & Weight

Dimensions (W X H X D): 85.2 x 118.1 mm (3-3/8 x 4-3/4 in.)  
Weight: 700g (24.7 oz.)

What's In The Box

Hood (model): ALC-SH147  
Lens front cap: ALC-F72S  
Lens rear cap: ALC-R1EM  
Case