# Clifton Cameras Product Specification

## Sony FE 100mm f2.8 STF GM OSS Lens Full Spec

Mount: Sony E-mount
Format: 35mm full frame
Focal Length (mm): 100
35mm Equivalent Focal Length (APS-C): 150
Lens Groups / Elements: 10-13 \*excluding APD element
Angle of View (35mm): 24°
Angle of View (APS-C): 16°1
Maximum Aperture (F): F2.8 (T5.6)
Minimum Aperture (F): F20 (T22)
Aperture Blades: 11
Circular Aperture: Yes
Minimum Focus Distance: 0.85m / 2.79 ft. (at "0.85m-∞" position); 0.57m / 1.87 ft. (at "0.57m-1.0m" position)
Maximum Magnification Ratio (X): 0.14 (at "0.85m-∞" position); 0.25 (at "0.57m-1.0m" position)
Filter Diameter (mm): 72
Image Stabilization (SteadyShot): Optical SteadyShot
Teleconverter Compatibility (X1.4): -
Teleconverter Compatibility (X2.0): -
Hood Type: Round shape, bayonet type

Size & Weight

Dimensions (W X H X D): 85.2 x 118.1 mm (3-3/8 x 4-3/4 in.)
Weight: 700g (24.7 oz.)

What's In The Box

Hood (model): ALC-SH147
Lens front cap: ALC-F72S
Lens rear cap: ALC-R1EM
Case